SECTION 27 13 23.13  
COMMUNICATIONS OPTICAL FIBER SPLICING AND TERMINATIONS

SPEC WRITER NOTES:

1. Delete between // // if not applicable to project. Also delete any other item or paragraph not applicable in the section and renumber the paragraphs.

PART 1 - GENERAL

1.1 DESCRIPTION:

This section specifies requirements for terminations of fiber optic cabling.

**1.2 SUMMARY**

Section Includes:

1. Termination Requirements.

**1.3 REFERENCES**

A. VA Infrastructure Standard for Telecommunications Spaces.

1.4 RELATED WORK:

A. Termination equipment: Section 27 11 19, COMMUNICATIONS TERMINATION BLOCKS AND PATCH PANELS.

B. Fiber optic cabling requirements: Section 27 13 23, COMMUNICATIONS OPTICAL FIBER BACKBONE CABLING.

* 1. SUBMITTALS:

A. Submit in accordance with Section 27 05 00, COMMON WORK RESULTS FOR COMMUNICATIONS SYSTEMS.

PART 2 - PRODUCTS

Not used.

PART 3 - EXECUTION

**3.1** **TERMINATION REQUIREMENTS.**

A. Terminate fiber optic cabling with // duplex Lucent connector (LC) adapters // // 12-fiber multi-fiber push on (MPO) connectors // // 24-fiber multi-fiber push on (MPO) connectors // as required for the application.

B. Pre-terminated connections are preferred for computer room structured cabling applications. Field termination (fusion splicing) for non-computer room applications where cable lengths cannot be determined in advance is acceptable.

‑ ‑ ‑ E N D ‑ ‑ ‑